
	SUMMARY OF COST FOR 

	CONSTRUCTION OF OFFICES AT

	COMSATS UNIVERSITY ISLAMABAD, ABBOTTABAD CAMPUS

	 
	Tender# CUI/ATD/45/Admin/Civil Work (2020-2021)

	 
	
	
	
	 

	 
	Sr.No.
	DESCRIPTION
	 
	TOTAL AMOUNT

	 
	
	
	
	 

	 
	
	
	
	 

	 
	1
	CIVIL WORKS
	Rs. = 
	                              -   

	 
	
	
	
	 

	 
	
	
	
	 

	 
	
	
	
	 

	 
	2
	PUBLIC HEALTH
	Rs. = 
	                              -   

	 
	
	
	
	 

	 
	
	
	
	 

	 
	
	
	
	 

	 
	3
	ELECTRICAL WORKS
	Rs. = 
	                              -   

	 
	
	
	
	 

	 
	
	
	
	 

	 
	
	
	
	 

	 
	
	GRAND TOTAL AMOUNT
	Rs. = 
	                                      -   

	 
	
	
	
	 

	 
	
	
	
	 

	 
	
	
	
	 

	 
	
	TOTAL COVERED AREA (SFT)
	 

	 
	
	
	
	 

	 
	
	
	
	 

	 
	
	COST PER SFT
	Rs. = 
	 

	 
	
	
	
	 

	 
	
	
	
	 

	 
	
	
	
	 

	 
	 
	 
	 
	 





	COMSATS UNIVERSITY ISLAMABAD ABBOTTABAD CAMPUS

	CONSTRUCTION OF OFFICES

	BILL OF QUANTITY

	CIVIL WORKS

	S#
	Description
	Qty
	Unit
	Rate
	Amount

	1
	Dismantling
	
	
	 
	 

	 
	Dismantling the existing upper portion of two columns for one feet height to over lap the reinforcement.  stacking of serviceable material and disposal of un-serviceable material surplus material of the project area from site as per instruction of the Engineer Incharge.
	2
	Lumsum
	 
	 

	2
	Excavation
	
	
	 
	 

	 
	Excavation in all kind of soil upto required depth for foundation and  etc. and stacking of excavated material clear of edge of excavation,  after excavation leveling and compaction  test including timbering shoring if required, back filling in layers and dewatering & compaction as specified and disposal of surplus excavated material out of project area any lead  as per drawings, technical provisions and instructions of the Engineer Incharge.
	250
	Cft.
	 
	 

	3
	Earth Filling
	
	
	 
	 

	 
	Supplying / filling local earth from approved  sources with all leads and lifts in or under floor,  including watering and consolidation by ramming in layers  not  exceeding 9" inch  depth leading to full compaction at least 95% AASHTO, (compacted measurement), as per drawings, technical provisions and instructions of the engineer incharge.
	200
	Cft
	 
	 

	4
	P.C.C (1:4:8)
	
	
	 
	 

	 
	Providing and laying 1:4:8 cement concrete using graded crushed stone 3/4" (19mm) down (Margalla crush) and down gauge and lawrancepur sand as per specification in foundation including levelling, compacting and curing etc. complete as directed by Engineer Incharge.
	
	
	 
	 

	a)
	Under foundation
	40
	Cft
	 
	 

	b)
	Under flooring
	85
	Cft
	 
	 

	5
	R.C.C (1:2:4)
	
	
	 
	 

	 
	Providing and laying reinforced cement concrete using screened crushed stone (Margalla) graded aggregate 3/4" (19mm) and down gauge and Lawarancepur sand as per specification having  a minimum  works cylinder crushing strength of 3000 lbs. per sq inch (psi) (21 MPa) at 28 days  with a mix not leaner than 1:2:4, including form work and its removal, compacting, leveling and curing etc. complete but excluding the cost of reinforcement as directed by the Engineer Incharge. 
	
	
	 
	 

	a)
	Column
	25
	Cft
	 
	 

	b)
	Beams & Lintels
	70
	Cft
	 
	 

	c)
	Slab
	25
	Cft
	 
	 

	6
	Cement  Concrete Floor
	
	
	 
	 

	 
	Providing and laying floor of 2" (50mm) thick 1:2:4 cement concrete using graded screened bajri 3/4"(19mm) and down gauge in ground floor laid in panels including form work, consolidation, steel trowel finished, and curing etc. Complete in all respects as per drawing and as directed by the Architect /Engineer Incharge.
	255
	Sft
	 
	 

	7
	Marble Patti
	
	
	 
	 

	 
	providing and laying 1/2" (13mm)thick  marble patties (panel strips) up to 1-1/2"(38mm) depth in floor  or as directed by the Engineer Incharge.
	140
	Rft
	 
	 

	8
	Reinforcement 
	
	
	 
	 

	 
	Providing and laying M.S deformed steel  reinforcement bars with minimum yield stress of 40000 Psi (grade 40)  including the cost of straightening, cutting, bending, binding, wastage, over laps, chairs and etc. complete in all kinds of R.C.C work and  as directed by the Engineer Incharge.
	240
	Kgs
	 
	 

	9
	Brick Masonry in Foundation 
	
	
	 
	 

	 
	Providing and laying first class solid burnt brick massonary set in cement mortor 1:5 for arches in straight or curved wall (9"to 22 1/2")  thick including scaffolding, form work and its removal, raking, out joints, and curing etc. complete in ground as directed by the Engineer Incharge.
	150
	Cft
	 
	 

	10
	Brick Masonry in Super Structure
	
	
	 
	 

	 
	Providing and laying first class solid burnt brick massonary (minimum crushing strength of brick 1200 psi.) set in cement mortor 1:5 for arches in straight or curved wall 9" to 13 1/2" (229 mm to 343 mm) thick including the cost of reinforcement 2 nos. #3 horizontal bars on every 4th course including straightening ,cutting ,bending ,binding wastage, overlaps, scaffolding, form work and its removal, raking, out joints, and curing etc. complete in ground as directed by the Engineer Incharge. 
	520
	Cft
	 
	 

	11
	Plaster Internal 
	
	
	 
	 

	 
	1/2" (13 mm) thick cement plaster 1:4 on soffits of ceiling cantilever slabs, sides and suffits of beams, slabs and R.C.C. wall etc. in ground floor including making edges, corner, curing and scaffolding etc. complete as directed by the Engineer Incharge.
	1100
	Sft
	 
	 

	12
	Plaster at Exterior Wall Surface
	
	
	 
	 

	 
	3/4" (19 mm) thick cement plaster 1:4 on soffits of ceiling cantilever slabs, sides and ,  and R.C.C. wall etc. in ground floor including making edges, corner, curing and scaffolding etc. including Providing and fixing chicken mesh with nails over all joints of wall with columns, beams and slab, complete as directed by the Engineer Incharge.
	720
	Sft
	 
	 

	13
	Plastic Emulsion
	
	
	 
	 

	 
	Painting with (ICI,Berger,Nipon or approved equivalent) Dulux Vinyl emulshion paint VIP of approved shade three coats over primer and including the cost of clearing the surface sand papering etc. and one primer coat (wall putty of ICI, Berger or approved equalent) complete over plastered surface at any height in any floor. or as directed by the Engineer incharge.
	1000
	Sft
	 
	 

	14
	Paint on Wood/Metal Surface
	
	
	 
	 

	 
	Providing and applying two coat of Paint on wood /Metal surface included primer prepering surface, filling with approved putty,rubbing,cleaning etc or as directed by the Engineer incharge
	180
	Sft
	 
	 

	15
	Weather shield 
	
	
	 
	 

	 
	Painting three coats of weather shield paint  (ICI/Berger/Nippon or approved equivalent)  of approved shade on plastered surface (External walls) including  projection soffits the cost of clearing the surface, sand papering etc. complete at any height in any floor and as directed by the Engineer Incharge.
	720
	Sft
	 
	 

	16
	Marble (Skirting)
	
	
	 
	 

	 
	Providing and fixing best quality  Boticina /Parlino marble or equivalent of approved colour in best quality size (30cm x 30cm x 2cm) and  (30cm x 15cm x 2cm) as approved equivalent, over (1:3) cement sand mortar  base under coat including, cutting, grinding and chemical polishing after fixing, complete in all respects, as per drawing or as directed by the Engineer Incharge.
	80
	Rft
	 
	 

	17
	Ceramic Tiles (Bath walls)
	
	
	 
	 

	 
	Providing and fixing glazed ceramics tiles in approved shade & colour (30cm x 45cm), (Master / Shabbir / Sonex or approved equivalent)  laid over 3/4" (19mm) thick cement mortar base 1:2 (one cement 2 sand) including fixing and  jointing, with colour grout mix and curing etc.complete in all respects, as per drawing or as directed by the Engineer Incharge.
	170
	Sft.
	 
	 

	18
	Matt Finish Tiles (Bath Floor)
	
	
	 
	 

	 
	Providing and fixing coloured glazed matt finish, non-skid tiles (30cm x 45cm), (Master  / Shabbir / Sonex or approved equivalent) laid over 1" thick cement sand mortar bed 1:2 (one cement 2 sand) including fixing and jointing, with colour grout mix and curing etc.design pattern, complete in all respects, as per drawing or as directed by the Engineer Incharge.
	80
	Sft.
	 
	 

	19
	Marble On Stairs
	
	
	 
	 

	 
	Providing and fixing approved quality Boticina / Parlino marble slab 2.5cm thickness with nosing as approved equivalent, pre-chemical polished approved colour,  on stair, laid over (1:3) cement sand mortar bed  under coat including, cutting, grinding at any floor, any height etc. complete in all respects, as per drawing and as directed by the Architect/ Engineer Incharge. 
	
	
	 
	 

	a)
	Tread 1"
	10
	Sft
	 
	 

	b)
	Riser 1/2" 
	5
	Sft
	 
	 

	20
	Solid (Flush) Door
	
	
	 
	 

	 
	Providing and fixing 1½" thick solid flush doors  with commercial ply 3mm on both faces of deodar wood shutter frame 1¼" thick and partal wood braces at about 3" apart and deodar wood lipping beading 1½" x 3/8" including brass hinges 5" long of approved best quality , including paint two coats with primer (ICI / Berger) except chowkat.Complete in all respects and as directed by Engineer Incharge.
	100
	Sft
	 
	 

	21
	Kick Plates
	
	
	 
	 

	 
	Providing and laying 22 gauge aluminium kick plate 24" (60cm) high fixed with screw 4" (10cm)  c/c on bottom rail of flush door only on commercial flush door. Complete in all respects as per drawings & specifications  and or as directed by Engineer Incharge.
	30
	Sft
	 
	 

	22
	Sliding Bolt
	
	
	 
	 

	 
	Providing and fixing of brass sliding bolt  of approved best quality for doors 10" long. Complete in all respects and as directed by Engineer Incharge.
	2
	Each
	 
	 

	23
	Tower Bolt
	
	
	 
	 

	 
	Providing and fixing of brass tower bolt  of approved best quality for doors 10" long. Complete in all respects and as directed by Engineer Incharge.
	4
	Each
	 
	 

	24
	Door Handle
	
	
	 
	 

	 
	Providing and fixing best quality door handle as per approval .Complete in all respects as per drawings & specifications  and or as directed by Engineer Incharge.
	10
	Nos.
	 
	 

	25
	Wooden Beeding 
	
	
	 
	 

	 
	P/F deodar wood beeding 2 1/2"x1/2" thick i/c hardware  (architrave )around the door chowkat with polishing etc.Complete in all respects as per drawings & specifications  and or as directed by Engineer Incharge.
	50
	Rft
	 
	 

	26
	MS / Steel Chowkats
	
	
	 
	 

	 
	Supply and fix steel chowkats press moulded 16 SWG for 9" & 4-1/2" th walls complete including hold fasts, ties for lateral movement P.C.C (1:2:4) caving filling etc including the cost of two coat of enamel paint.and one coat of primer red oxide
	75
	Rft
	 
	 

	27
	Suspended Acoustic Ceiling
	
	
	 
	 

	 
	Providing & fixing 2' x 2' acoustic boards NRC range 0.80 with powder coating imported aluminium channels with galvanized steel wires 12 SWG hanging system, complete in all respects and as directed by the Architect / Engineer Incharge.
	260
	Sft
	 
	 

	28
	Steel  Windows & Ventilator
	
	
	 
	 

	 
	Supply and fixing the 16 SWG steel tube pipe/box sectios not exceeding 1.48Sqm super each with openable /fixed panels frame sections sashes with all necessary steel fitting/iron mongrey ,holdfast etc, and two coats of sythentic enamel paint but except glass panes and wire gauze and including 5mm glass complete in all respect.
	80
	Sft.
	 
	 

	29
	Iron Grills (Safety Grill)
	
	
	 
	 

	 
	Supply and fix guard bars, grills, railing, hooks, hold fast and frames etc; cut to dead length, reduced to size, shape, figure etc; including punching/drilling holes if necessary and fixing, assembling by welding or with the use of bolts, nuts, rivets washers etc; and erection/fixing in position including making good the disturbed surfaces including the one coat of primer/rust proof and two coat of enamel paint (ICI, Berger , Nipon or approved equivalent) as per design  and direction of Engineer Incharge.
	72
	Sft
	 
	 

	30
	Rain Water Pipe
	
	
	 
	 

	 
	Providing and fixing 4" (100 mm) dia UPVC (Dadex or approved equivalent) rain water down pipe with bolts and fixed in cement concrete 1:2:4 including the cost of all fitting etc.complete in all respects, as per drawing or as directed by the Engineer Incharge.
	10
	Rft
	 
	 

	31
	Truss
	
	
	 
	 

	 
	Providing and installing for complete steel structural works  with trusses, beams, gurders, joists, cleasts, angles, purlins, tee section , gusset plates , base plates , bolts  and channel with all required accessories and one coat of red oxide and two coats of enamel (ICI , Berger or approved equivalent) paints etc.as specified and as shown on the drawings . Complete in all respect as per drawings, plans and or as directed by the Engineer Incharge .
	300
	Kgs
	 
	 

	32
	Galvanized Corrugated Steel Sheet
	
	
	 
	 

	 
	Providing, fabricating and fixing in position, galvanized corrugated steel sheets, 26 SWG in thickness, including steel and rubber washers ‘J’ bolts and nuts over roof sheeting and trusses  complete in all respects as per drawings or as directed by the Engineer.
	420
	Sft
	 
	 

	33
	Facia Board
	
	
	 
	 

	 
	Providing and installing of Facia boards complete comprising of M.S pipe frame 1"x1" 20 SWG including threee coats of enamel paint and covered with 26 SWG prepainted coloured M.S sheet with all required accessories etc. as specified and as shown on the drawing complete in all respect  or as directed by the Engineer.
	90
	Sft
	 
	 

	34
	Water Drainage Gutter
	
	
	 
	 

	 
	Providing, fabricating and fixing in position, galvanized plain sheet water drainage gutters 6" radius, 20 SWG in thickness including steel and rubber washers  bolts and nuts to specified geometry including end receiving box complete in all respects as per drawings or as directed by the Engineer.
	25
	Rft
	 
	 

	
	Total Amount
	
	
	
	                 -   

	
	
	
	
	
	



	COMSATS UNIVERSITY ISLAMABAD ABBOTTABAD CAMPUS

	CONSTRUCTION OF OFFICES

	BILL OF QUANTITY

	PUBLIC HEALTH  WORKS

	S#
	Description
	Qty
	Unit
	

	
	
	
	
	Rate
	Amount

	 
	FITTING AND FIXTURES:-
	
	
	
	

	1 
	Supply and fix water closet Asiatic pattern best quality Shabir, Master or equivalent complete with closet foot rest (white) 13 liters flushing cistern low down flush pipe etc; any size or mark, fixed to concrete, brick, stone, or woodwork, Pak made in white colour (Export quality or equivalent).
	2
	No.
	
	

	 
	 
	
	
	
	

	2 
	Supply and fix wash hand basin in light colour with pedestal glazed ware 650mm long, one hole complete with waste pipe, coupling, chain and plug, best quality Pak made Shabir, Master or Equlant fixed to concrete, brick, stone or woodwork.Pak made Shabir, Master or Equlant (Export or equivalent quality).
	2
	No.
	
	

	 
	 
	
	
	
	

	3 
	Supply and fix towel rail, chromium plated, single rod any pattern, shape and size Pak made complete with plugs, screws etc fixed to concrete, stone, brick or woodwork.
	2
	No.
	
	

	 
	 
	
	
	
	

	 
	 
	
	
	
	

	4 
	Supply and fix soap/sponge tray any shape pattern and size Pak made complete with plugs, screws etc fixed to concrete, stone or woodwork.
	2
	No.
	
	

	 
	 
	
	
	
	

	5 
	Supply and fix toilet paper holder any shape pattern and size foreign made complete with plugs, screws etc foxed to concrete, stone or woodwork.
	2
	No.
	
	

	 
	 
	
	
	
	

	6 
	Water taps 1/2" dia heavy pattern chromium plated screw in any type complete of Baig/Faisal/Asia.
	2
	No.
	
	

	 
	 
	
	
	
	

	7 
	Supply and fix mirror any shape and pattern 5mm thick of sizes, Balgium made edges ground, complete fixed to concrete, brick, stone or woodwork including Aluminum frame and Lasany wood used on the back of the mirror.
	8
	Sft
	
	

	 
	 
	
	
	
	

	8 
	Bib cock Master chromium plated fancy type screwed down BSP, 15mm dia supply and fixing.
	12
	No.
	
	

	 
	 
	
	
	
	

	 
	 
	
	
	
	

	9 
	Supply and fix 100mm dia  floor trap including reducer etc complete.
	2
	No.
	
	

	 
	 
	
	
	
	

	10 
	Supply and fix casted grating chromium plated 100mm x 100mm.
	2
	No.
	
	

	 
	 
	
	
	
	

	11 
	Excavation for pipe lines, trenches and structures upto any depth in all type of size including back filling with excavated materials compacting ramming including shoring de-watering if any required and disposal of surplus earth to areas as specified, spreading, levelling and dressing etc. complete as per drawings and technical provisions.
	30
	Cft
	
	

	 
	 
	
	
	
	

	12 
	Providing and fixing  of class "D" Upvc Dadex or approved equivalent vent pipe of best quality sanitary waste , vent etc pipe including sockets, bends, Tees etc. complete as approved by the Engineer Incharge.
	
	
	
	

	 
	a)   75 mm dia
	30
	Rft
	
	

	 
	b) 100 mm dia
	25
	Rft
	
	

	 
	c) 150 mm dia
	40
	Rft
	
	

	 
	 
	
	
	
	

	13 
	Providing and construction manhole  size 1.5 feet x 1.5 feet  (inside dimensions) x 1.5 feet deep as per approved design and specifications complete 4 inches to 12 inches , with R.C.C (1:2:4) top slab 3" thick ,8 inches thick solid block masonry walls cement mortar (1:4) 4 inches thick P.C.C (1:2:4) in foundation,1/2 inch (13mm) thick cement plaster in 1:4 c.m. to both sides wall surfaces, including the cost of excavation, back filing, disposal of excavated stuff Complete in all respects, as per drawing and as directed by the Engineer Incharge.
	1
	No.
	
	

	 
	 
	
	
	
	

	14 
	Supply and fix manhole cast iron cover with frame 450mm circular or rectangular set in cement mortar and haunching in concrete as specified.
	1
	No.
	
	

	 
	 
	
	
	
	

	 
	WATER SUPPLY INSTALLATIONS:-
	
	
	
	

	15 
	Cold  Water Supply
	
	
	
	

	 
	Providing and Laying DADEX  'PPR' pipe with all fittings (i.e. sockets, bends, tees, elbows where required) and laid complete in trenches (exclusive of excavation) or fixed to walls, ceilings and floors etc including caps and plugs as required  supply and fixing.
	
	
	
	

	 
	a) 25mm  dia
	170
	Rft.
	
	

	 
	b) 20mm dia
	45
	Rft.
	
	

	 
	 
	
	
	
	

	16 
	Hot  Water Supply
	
	
	
	

	 
	Providing and Laying DADEX  'PPR' pipe with all fittings (i.e. sockets, bends, tees, elbows where required) and laid complete in trenches (exclusive of excavation) or fixed to walls, ceilings and floors etc including caps and plugs as required  supply and fixing.
	
	
	
	

	 
	a) 25mm  dia
	30
	Rft.
	
	

	 
	b) 20mm dia
	30
	Rft.
	
	

	 
	 
	
	
	
	

	17 
	Gunmetal Valve
	
	
	
	

	 
	Providing and fixing full way gun metal valves with threaded or flanges ends  with rubber washer for smooth operation  quality or as approved by the Engineer Incharge.
	
	
	
	

	 
	 
	
	
	
	

	 
	a) 25mm dia valve
	1
	No.
	
	

	 
	b) 20mm dia valve
	1
	No.
	
	

	 
	 
	
	
	
	

	18 
	Over Head Water Tank
	
	
	
	

	 
	Providing  and fixing  of Master or approved equivalent fiber glass water tank (Double ply) at top roof, including cost of  P.P.R.C. pipes, valves (washout, air release, inlet and outlet) sleeves, specials,  float valve cover, etc. with all fitting complete approved quality including testing, complete in all respect as per drawings and as directed by the Engineer incharge.
	
	
	
	

	 
	300 Gallon
	1
	No.
	
	

	
	Total Amount
	
	
	
	-








	COMSATS UNIVERSITY ISLAMABAD ABBOTTABAD CAMPUS

	CONSTRUCTION OF OFFICES

	BILL OF QUANTITY

	ELECTRICAL WORKS

	S#
	Description
	Qty
	Unit
	

	
	
	
	
	Rate
	Amount

	E-01
	Supply, installation, testing & commissioning of circuit wiring from distribution board to the nearest switch board point to be wired with 3xsingle core 2.5mm sq (7/.029) PVC insulated 300/500 volt grade copper wire (Phase Neutral & Earth) in and including cost of appropriate size of heavy duty PVC conduit (min size 20mm dia) recessed in walls, columns, floors, slabs or as required as per site conditions complete with all PVC conduit accessories such as pull boxes, junctions boxes, sockets, bends, steel pull wire and complete in all respects. Each circuit shall have independent insulated green colour copper wire as earth conductor. 
	2
	Job
	 
	 

	 
	 
	
	
	 
	 

	E-02
	Wiring for one light point controlled by one switch and wired with 3xsingle core 1.5mm sq (3/036) PVC insulated, 300/500 volt grade copper wire (Phase & Neutral) in and including cost of appropriate size of heavy duty PVC conduit (min size 20mm dia) partly shared recessed in walls, columns, floors, slabs or as required as per site conditions including all conduit accessories such as steel pull boxes, PVC junction boxes for ceiling and wall, sockets & bends also steel pull wire. Complete in all respects with final testing and commissioning.
	4
	Point
	 
	 

	 
	 
	
	
	 
	 

	E-03
	Same as item E-02 mentioned above but for ceiling fans including cost of fan hook as per sketch/drawing attached and as approved by Engineer Incharge.
	2
	Point
	 
	 

	 
	 
	 
	
	
	 
	 

	E-04
	Same as item E-02 mentioned above but for Exhaust Fan
	2
	Set
	 
	 

	E-05
	Same as item E-02 mentioned above but wiring for one 3 pin 5 AMP  socket from nearest switch board or from nearest 15 Amp socket . Complete in all respect with final testing and commissioning.
	2
	Each
	 
	 

	 
	 
	
	
	 
	 

	E-06
	Wiring for one 3 pin 15 AMP socket  direct from DB with 3xsingle core 4mm sq (7/036) PVC insulated, 300/500 volt grade copper wire (Phase, Neutral & Earth) in and including cost of 25mm dia heavy duty PVC conduit recessed in walls, columns, floors, slabs or as required as per site condition including all conduit accessories such as sockets, bends, steel wire pull boxes and complete in all respects with final testing and commissioning.
	2
	Each
	 
	 

	 
	 
	
	
	 
	 

	E-7
	Supply and installation of 5 amps piano type switch gang plate as specified & approved by Engineer-in-Charge with appropriate size of back steel box 16SWG with earth terminal, two coats of antirust paint fixed recessed in wall including all fixing accessories and of following types:
	
	
	 
	 

	 
	b.
	2 – gang switch plate
	2
	Each
	 
	 

	 
	c.
	3 – gang switch plate
	2
	Each
	 
	 

	 
	d.
	 4 – gang switch plate
	1
	Each
	 
	 

	 
	 
	
	
	 
	 

	E-8
	Supply and installation Hum free regulator as specified and approved by Engineer-in-Charge  complete with  back steel box of appropriate size with two coats of antirust paint fixed recessed in wall including all fixing accessories.
	2
	Each
	 
	 

	 
	 
	
	
	 
	 

	E-9
	Supply and installation of 3 pin switch socket combined unit as specified and approved by Engineer-in-Charge with appropriate size of back steel box 16SWG, two coats of antirust paint, fixed recessed to walls or ceiling including all fixing accessories and of the following types:-
	
	
	 
	 

	 
	a.
	3 pin 5Amps switch socket unit
	2
	Each
	 
	 

	 
	b.
	3 pin 15Amps switch socket unit
	2
	Each
	 
	 

	 
	 
	
	
	 
	 

	E-10
	Supply, installation testing and commissioning of  spot light light fixture ceiling mounted complete with housing, holder and with 18 watt comptalux lamp and as approved by Engineer-in-Charge/Architect.
	4
	Each
	 
	 

	 
	 
	
	
	 
	 

	E-11
	Supply, installation, testing and commissioning of LED light 40 watt recessed in wall complete in all respects.
	2
	Each
	 
	 

	 
	 
	
	
	 
	 

	E-12
	Supply, installation, testing and commissioning of ceiling fans, AC capacitor type complete with hanging  rod, canopy, blades, nuts and bolts and of specified make including cost of all necessary materials and complete in all respects and of the following sizes:
	
	
	 
	 

	 
	 
	  56" Sweep
	2
	Each
	 
	 

	 
	 
	
	
	 
	 

	E-13
	Supply, installation, testing and commissioning of exhaust fans of following sizes complete with frame and of specified make including cost of all necessary materials and complete in all respects with all civil works such as dismantling and making good the same as directed by Engineer-in-Charge and also including fly-mesh/louvre as approved by Engineer-in-Charge:
	
	
	 
	 

	 
	 
	 12" dia with steel body
	2
	Each
	 
	 

	 
	 
	
	
	 
	 

	E-14
	Supply, installation, testing and commissioning of multicore, stranded conductor copper cable, 600/1000 volt grade PVC, insulated, PVC sheathed as specified in pre-laid conduit, trenches or on cable trays as per route shown on drawings or as directed by Engineer-in-Charge including cost of all necessary materials, termination at both ends, cable lugs and of the following sizes:
	
	
	 
	 

	 
	Multicore, Nonarmoured, PVC insulated & PVC Sheathed
	
	
	 
	 

	 
	a.
	1 x 4 core 16mm sq
	70
	Rft
	 
	 

	 
	b.
	1 x  4 core 25mm sq
	25
	Rft
	 
	 

	 
	 
	
	
	 
	 

	E-15
	Supply, installation, testing of PVC heavy duty conduit as specified concealed in RCC slabs, walls, floors columns or fixed to slab, wall above false ceiling as per site conditions including cost of all conduit accessories, steel pull boxes, pull wire, junction boxes and complete in all respects and of the following sizes:
	
	
	 
	 

	 
	a.
	25mm (1") dia
	30
	Rft
	 
	 

	 
	c.
	50mm (2") dia
	50
	Rft
	 
	 

	E-16
	SUB-MAIN PANEL BOARD
	
	
	 
	 

	 
	 
	
	
	 
	 

	 
	Supply, installation, testing and commissioning of factory fabricated Sub-Main Panel Boards free standing/wall mounted type made of M.S sheet 14 SWG degreased, derusted, zinc phosphated finished with electrostatic powder coating, of approved colour with hinged door, lockable handle, protection plate, earth and neutral strip, complete internally wired, flexible earthing strap for door manufactured by any one of the approved manufacturers as specified and comprising as under:
	
	
	 
	 

	 
	SMPB -N
	1
	Nos.
	 
	 

	 
	 INCOMING
	
	
	 
	 

	-
	1x80 AMP, TP, MCCB, 25KA with O/L & S/C Protection.
	
	
	 
	 

	-
	4 x copper busbars of 100 AMP ratings.
	
	
	 
	 

	-
	Digital Voltmeter with phase selector switch 
	
	
	 
	 

	-
	Indication lights Red, Yellow, Blue.
	
	
	 
	 

	 
	OUTGOING
	
	
	 
	 

	 
	2 x 60 AMP, TP, MCCB, 15KA with O/L & S/C Protection.
	
	
	 
	 

	 
	1 x 40 AMP, TP, MCCB, 15KA with O/L & S/C Protection.
	
	
	 
	 

	
	
	
	
	
	 Total Rs. 
	                -   



[image: ][image: ]
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