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CUI/ATD/02/Admin/Sound System (2021-2022)

	S. No.
	Description
	Quantity

	1
	Technical Specification of Sound System Required for Auditorium 
Dimensions of Hall 80’ x 136’ H17’ and Stage 56’ x 23’ H14’

	Complete Set

	1.1
	Audio Amplifier (professional)
· Mixture amplifier for paging and background music system
· Power rated 240 W or better
· Minimum Three Mic inputs by phone jack type
· Minimum Two Aux Inputs and 2 line inputs for spare use:
· Best Input Sensitivity Impedance for all mics. 
· 2 EMC priority inputs
· 70V, 100V and low impedance 4-19ohm speaker output or better
· Best Output Sensitivity & Impedance: MIX OUT
· Best suitable Frequency Response for all mics and Auxiliary 
· Best suitable Gain Control: ±2.5mV~ 75mV at 30db
· Best suitable Phantom Power: +48V, with LED indicator
· Short circuit overload and high temp protection
· 3U Rack Mount
· Faults monitoring module
· Body: Aluminum plate, steel plate 
Or equivalent with one year replacement / parts warranty on site.
	04

	1.2
	Audio Pre-Mixer
· Digital audio pre-mixer with microphone 16 inputs
· -20dB attenuation per channel
· Dual-channel independent control of 7-segment EQ
· MP3 player
· External Line Returns (XLR) inputs and Phono Inputs
· Slider Volume Levels and Master Slider Control
· 16/99 two digital effects
· With auxiliary transmission, auxiliary return function
· 48V Phantom Power Selection or better
· 3-band equalizer for warm sound
· Built-in power amplifier at 2*350W at 4 ohm  
Or equivalent with one year replacement / parts warranty on site.
	02

	1.3
	Passive Wall Mount Speaker
· Built-in 100v/70v transformer
· Wall mount type loudspeaker
· High-voltage, low-current mode, which makes longer distance transmission and parallel connection of multiple loudspeakers possible.
· RMS Watts and Peak Watts in accordance to the Auditorium Dimensions and compatible with Amplifier
· Or equivalent with one year replacement / parts warranty on site.
	18

	1.4
	Ceiling Speaker
· Built-in 100v/70v transformer
· RMS Watts and Peak Watts in accordance to the Auditorium Dimensions and compatible with Amplifier preferably Power taps 3W & 5W @100V or better
· Capacity to reduces line losses on longer distance and allows easy parallel connection of multiple loudspeakers.
· wide frequency response 100-13kHz,
· Metal grille, ABS baffle & back cover with Flush-mount dog ears
· Compatible with Auditorium already installed Ceiling, white color
Or equivalent with one year replacement / parts warranty on site.
	20

	1.5
	Professional Heavy-duty Speaker System
· Minimum 350W RMS - 700W Program / 1400W Peak
· 15″ woofer
· Best feasible, Frequency boost switch
· Speak on and 6.3mm jack connections
· Signal and Protect LEDs
· Durable carpet covering
· Dual angle pole mounts
Or equivalent with one year replacement / parts warranty on site.
	02 pair

	1.6
	Power Amplifier
· Thermal, overcurrent, DC and output short protect circuitry
· Speakon outputs
· XLR outputs to link other audio equipment
· XLR inputs
· Built-in switchable limiter
· Continuously variable speed fan
Or equivalent with one year replacement / parts warranty on site.
	02 pair

	1.7
	Digital Audio Cordless Microphone Set
· Wireless UHF Microphone Set
· Wireless Collar & Handheld microphone set
· Digital Select-able frequencies
· Each set has 2 Microphones with Wireless collar & Hand held microphone
Or equivalent with one year replacement / parts warranty on site.
	04 set

	1.8
	Goose Neck Cable Microphones for Head table and Dice)
· Anti-mobile phone interference
· Cable LED goose neck microphone
· Ring LED to indicate power on/off status
· Or equivalent with one-year replacement / parts warranty on site.
	08

	1.9
	With Voltage control / power surge management over normal and Generator system
	01

	1.10
	Imported high quality Microphone Cable 
	02 Rolls

	1.11
	Imported high quality 2 core Speaker Cable 
	03 Rolls

	1.12
	Imported high quality XLR jack (male/female) connector 
	12 Pairs

	1.13
	Imported high quality Phono Jack connector 
	04 Pairs

	1.14
	High Quality Equipment Rack
	02

	1.15
	High quality Computer Sound Connectors
	04 Pairs



The bidders are required to visit the venue / premises before participating in the tender to get clear vision and requirements. The turn-key integrated auditorium sound system must achieve high quality of service with noise free, distortion free and echo free solution where sound distributed equally in the auditorium with voltage control stabilizer with more controls for creating equipment-based sound zones. 
Note: Separate Marks will be given to those vendors / service providers, who will visit the location before submitting the tender document (bid).
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