CUI/ATD/10/LiScent/RO Plant (2021-2022)
	Sr. No.
	Items Specifications
	Required Quantity

	01
	Supply and installation of RO Plant for drinking water with 3000GPD (Gallon per day)
Technical Specifications:
· Water Producing Capacity: 3000GPD (Gallon per day) with mineral dosing Ca, Mg, Na, K with WHO Specification.
· Output water pH 6.5-8.5.
· Filling Station Table (Auto/Manual).
· Bottles for filling of 5 gallons capacity (100 PCS Food grade Material).
· Turbidity: 3.0 NTU
· Working Environment: 5°C -45°C.
· Voltage: 220V, 50Hz.
· Effluent Standards: Feed water conductivity <1000us/cm, water conductivity S10us/cm (desalting rate is 98-99.8%)
· Manufacturer Warranty: One Year
· Supply and Installation
· Installation Conditions: Interior Installation
· After Sale Services required.
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