Tender#: CUI/ATD/35/ES (2020-2021)
	S#
	Description
	Quantity

	1
	[bookmark: _GoBack]Portable Pumping Gas Detector (NO & NO2) NOX Meter:
· Measuring Range 0-100 ppm.
· Resolution: 0.01 ppm
· Precision is 2-3% FS
· Alarm with sound, light and vibration, alarm point is settable.
· Large Capacity of lithium polymer battery.
· Detect NO and NO2 gas concentration in the air.
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