Tender#: CUI/ATD/42/TWAS (2020-2021)
	S. No
	Description
	Quantity

	1
	Nitrogen Argon Inert Atmosphere Muffle Furnace (with Vacuum Pump)

Specification:
· Chamber Size: L150x W150 x H200 mm
· Double Stainless Steel Chamber with fan cooling system.
· Max Temp 1200oC, Working Temperature 1100oC
· Kanthal / NiCr wire Heaters
SSR Digital PID controlled heating system, Vacuum 0.1Mpa [1Bar] Max, Gas inlet/outlet/safety valve, gas pressure gauge, Rota  flow equipped, over temp safety cutout. 
· Vacuum pump 0.1Mpa.
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