Re-Tender: CUI/ATD/07/Hostel/Bed & Cupboard

	Sr. No.
	Items Specifications  
	Required Quantity

	01
	Single Beds: 
Size L74xW38xH20’’ Extra Height at Pillow Side 9’’, Frame of MS Pipe 16 Square Gauge 1’’x2/12’’, Seventeen Iron Rods between frame sizes of iron rods 1’’x5’’’. The distance between iron rods should be 3’’. Bed Foot made of Iron Pipe 16 Square gauge 2’’x 2’’. Two Rods at Pillow side size 1’’x1’’. 3’x74 Ply sheet on Bed. The bed should be painted with white enamel paint.
	100 No

	02
	Cupboard Iron: 6’x3’ x 1 ½’ with hanging and showcase rack two door with chapka lock, 24 Square Gauge   iron sheet with blue enamel paint.
	15 No

	03
	Study Table: 
Size 3’x2’x2 ½’ 1 1/2'’ X1 ½’’ x 1 ½’’ Ms Pipe Structure, 18 Gauge Ms Pipe, Top 16 mm Thick MDF Lamination Sheet, Frame of Table with Painted (As per sample) 
Frame: 18 gauge
	15 No





